South Australia
Electrical Products (Part 2 Declarations) Variation Proclamation 2009
under section 5 of the Electrical Products Act 2000

Part 1—Preliminary
1—Short title
This proclamation may be cited as the Electrical Products (Part 2 Declarations) Variation Proclamation 2009.
2—Commencement
This proclamation comes into operation on the day on which it is made.
3—Variation provisions
In this proclamation, a provision under a heading referring to the variation of a specified proclamation varies the proclamation so specified.

Part 2—Variation of Electrical Products (Part 2 Declarations) Proclamation 2004
4—Variation of Schedule 1—Safety and performance labelling
	(1)	Schedule 1, item 7—delete the item and substitute:

7	Clothes dryer, being an electrical appliance that—
	(a)	is a household type; and
	(b)	is for drying textile material,
but does not include a heated towel rail.	
	(2)	Schedule 1, item 8—after paragraph (b) insert:
	(ba)	is portable; and
	(3)	Schedule 1, item 12(c)—after "lamps" wherever occurring insert:
(including Light Emitting Diode "LED" types)
	(4)	Schedule 1, item 35(c)—delete paragraph (c) and substitute:
	(c)	has a rating not exceeding 20A,
	(5)	Schedule 1, item 43—before "but does not include" insert:
and includes an appliance that accommodates 1 or more heat lamps,
	(6)	Schedule 1, item 45(d)—delete paragraph (d) and substitute:
	(d)	has a rating not exceeding 20A,
	(7)	Schedule 1, item 48(a) and (b)—delete paragraphs (a) and (b) and substitute:
	(a)	is a transportable spa pool or transportable spa bath; or
	(ab)	is for circulating air or water in a conventional bath; or
	(b)	is for use in the operation or cleaning of a swimming pool, non‑transportable spa pool or non‑transportable spa bath,
5—Variation of Schedule 2—Energy performance registration
	(1)	Schedule 2—before item 1 insert:

A1	Air‑conditioner—close control, being a unitary air‑conditioner that—
	(a)	is designed for high sensible heat ratio applications; and
	(b)	is capable of maintaining close control of both temperature and humidity; and
	(c)	consists of 1 or more factory‑made assemblies that—
	(i)	includes a compressor, direct expansion evaporator, air‑moving device and air‑filtering device; and
	(ii)	may include a condenser, humidifier or reheating function.	AS/NZS 4965.22	
	(2)	Schedule 2, item 2—delete "AS/NZS 38231" and substitute:
AS/NZS 3823.21
	(3)	Schedule 2, item 4—delete "AS/NZS 1359.102.32" and substitute:
AS/NZS 1359.52
	(4)	Schedule 2—after item 4 insert:

4A	External power supply, being an electrical device that—
	(a)	has an input from mains supply (usually 115V/60Hz, 230V/50Hz, 240V/50Hz or a range including some or all of those input conditions); and
	(b)	has 1 extra low voltage output (either ac or dc) that is either at a fixed voltage or user selectable through a selector switch; and
	(c)	is sold with, or intended to be used with, a separate end‑use product that constitutes the primary load; and
	(d)	is contained in a separate physical enclosure from the end‑use product (that is, the housings of the power supply and its associated product are different, not their retail packaging); and
	(e)	is connected to the end use product via a hard‑wired or removable male/female electrical connection, cable, cord or other wiring; and
	(f)	does not have batteries or battery packs that physically attach directly to the power supply unit (including those that are removable, for example, a battery pack for a portable electric drill); and
	(g)	does not have a battery chemistry or type selector switch and an indicator light or state of charge meter,
but does not include an appliance of the type referred to in clause 1.2 of AS/NZS 4665.2.	AS/NZS 4665.22	
	(5)	Schedule 2, item 5—delete "AS/NZS 47832" and substitute:
AS/NZS 4783.21
	(6)	Schedule 2, item 6—delete "AS/NZS 44741" and substitute:
AS/NZS 4474.21
	(7)	Schedule 2, after item 6 insert:

6A	Incandescent lamp, being—
	(a)	a GLS (general lighting service) incandescent lamp with a nominal voltage of 220V or more, a nominal wattage of less than 150W and with the attributes set out in clause 1.1.2 of AS/NZS 4934.2(Int): 2008, but not including a primary coloured lamp; or
	(b)	an ELV (extra low voltage) halogen non‑reflector type lamp (a gas filled lamp containing halogens or halogen compounds) with a filament consisting of tungsten, a nominal voltage of between 5 and 14V inclusive and with the attributes set out in clause 1.1.3 of AS/NZS 4934.2(Int): 2008,
but does not include a lamp of the type referred to in clause 1.2 of AS/NZS 4934. 2(Int).	AS/NZS 4934. 2(Int)2	
	(8)	Schedule 2, item 7—delete "AS/NZS 47822" and substitute:
AS/NZS 4782.22
	(9)	Schedule 2—after item 7 insert:

7A	Liquid‑chilling package, being electrical equipment that—
	(a)	has a cooling capacity of 350kW or more; and
	(b)	is a factory made and prefabricated assembly (not necessarily shipped as 1 package); and
	(c)	has 1 or more compressors, condensers and evaporators; and
	(d)	has interconnections and accessories; and
	(e)	is designed for the purpose of cooling water; and
	(f)	is specifically designed to make use of a vapour compression refrigeration cycle to remove heat from water and reject the heat to a cooling medium, usually air or water.	AS/NZS 4776.22	
	(10)	Schedule 2, item 9—delete "AS/NZS 44741" and substitute:
AS/NZS 4474.21
	(11)	Schedule 2, item 10—delete "AS/NZS 44741" and substitute:
AS/NZS 4474.21
	(12)	Schedule 2—after item 10 insert:

10B	Set top box, being an electrical appliance that is used to convert digital television signals to a signal compatible with the existing audiovisual display technology, including the following:
	(a)	analogue radio frequency;
	(b)	composite video;
	(c)	super video;
	(d)	component video;
	(e)	digital interface;
	(f)	high definition multimedia interface,
but does not include an appliance of the type referred to in clause 1.2 of AS/NZS 62087.2.	AS/NZS 62087.22	
10C	Television set, being an electrical appliance for the display and possible reception of television broadcast and similar services for terrestrial, cable, satellite and broadband network transmission of analogue and/or digital signals.	AS/NZS 62087.2.21	
	(13)	Schedule 2, item 11—delete "AS/NZS 46922" and substitute:
AS/NZS 4692.22
6—Variation of Schedule 3—Energy efficiency labelling
	(1)	After item 3 insert:

3A	Fluorescent lamp ballast (within the meaning of Schedule 2)	
	(2)	After item 6 insert:

6A	Television set (within the meaning of Schedule 2)	
Made by the Governor's Deputy
with the advice and consent of the Executive Council
on 22 October 2009
MEN09/013